1. Avilable in Top mount, Side mount & Overhung top mount options.
2. Post dimensions : Various options available , (1”X2”, 1 1/2”/2”, 2”/2”) .
3. Extruded screw spline joinery .
4. Interior or Exterior glazed panels Available for 6mm & 8mm glasses .
5. Available with multiple top rail designs.
6. Finish in Duracron, Acrynar, Duranar (XL) and Anodized.
7. Ideal for high rise buildings.
8. Available in standard & Premium glass.
9. i.e. – clear, tinted, acid etched, patterned, digitally printed (Bird friendly)

In compliance with OBC and CSA standards.